| Parola for Arduino 3.5 Text effects for LED Matrix modular hardware

MD_PZone Member List

This is the complete list of members for MD_PZone, including all inherited members.

addChar(uint16_t code, uint8_t *data) | MD_PZone |
begin(MD_MAX72XX *p) | MD_PZone |
delChar(uint16_t code) | MD_PZone |
getCharSpacing(void) | MD_PZone |
getIntensity() | MD_PZone |
getInvert(void) | MD_PZone |
getPause(void) | MD_PZone |
getScrollSpacing(void) | MD_PZone |
getSpeed(void) | MD_PZone |
getSpeedIn(void) | MD_PZone |
getSpeedOut(void) | MD_PZone |
getStatus(void) | MD_PZone |
getSynchTime(void) | MD_PZone |
getTextAlignment(void) | MD_PZone |
getTextExtent(uint16_t &startColumn, uint16_t &endColumn) | MD_PZone |
getTextWidth(const uint8_t *p) | MD_PZone |
getZone(uint8_t &zStart, uint8_t &zEnd) | MD_PZone |
getZoneEffect(zoneEffect_t ze) | MD_PZone |
getZoneExtent(uint16_t &startColumn, uint16_t &endColumn) | MD_PZone |
getZoneFont(void) | MD_PZone |
isAnimationAdvanced(void) | MD_PZone |
MD_PZone(void) | MD_PZone |
setCharSpacing(uint8_t cs) | MD_PZone |
setIntensity(uint8_t intensity) | MD_PZone |
setInvert(uint8_t invert) | MD_PZone |
setPause(uint16_t pause) | MD_PZone |
setScrollSpacing(uint16_t space) | MD_PZone |
setSpeed(uint16_t speed) | MD_PZone |
setSpeedInOut(uint16_t speedIn, uint16_t speedOut) | MD_PZone |
setSpriteData(const uint8_t *inData, uint8_t inWidth, uint8_t inFrames, const uint8_t *outData, uint8_t outWidth, uint8_t outFrames) | MD_PZone |
setSynchTime(uint32_t zt) | MD_PZone |
setTextAlignment(textPosition_t ta) | MD_PZone |
setTextBuffer(const char *pb) | MD_PZone |
setTextEffect(textEffect_t effectIn, textEffect_t effectOut) | MD_PZone |
setZone(uint8_t zStart, uint8_t zEnd) | MD_PZone |
setZoneEffect(boolean b, zoneEffect_t ze) | MD_PZone |
setZoneFont(MD_MAX72XX::fontType_t *fontDef) | MD_PZone |
zoneAnimate(void) | MD_PZone |
zoneClear(void) | MD_PZone |
zoneReset(void) | MD_PZone |
zoneShutdown(bool b) | MD_PZone |
zoneSuspend(bool b) | MD_PZone |
~MD_PZone(void) | MD_PZone |