| Parola for Arduino 3.0 Text effects for LED Matrix modular hardware

Macros
MD_Parola_lib.h File Reference

Contains internal library definitions. More...

This graph shows which files directly or indirectly include this file:

## Macros
#define | DEBUG_PAROLA 0
| Set to 1 to enable General debug output.
#define | DEBUG_PAROLA_FSM 0
| Set to 1 to enable Finite State Machine debug output.
#define | TIME_PROFILING 0
| Set to 1 to enable Time Profile debug output.
#define | PRINT(s, v)
| (GENERAL) Print a string followed by a value (decimal)
#define | PRINTX(s, v)
| (GENERAL) Print a string followed by a value (hex)
#define | PRINTS(s)
| (GENERAL) Print a string
#define | FSMPRINT(s, v)
| (FSM) Print a string followed by a value (decimal)
#define | FSMPRINTX(s, v)
| (FSM) Print a string followed by a value (hex)
#define | FSMPRINTS(s)
| (FSM) Print a string
#define | PRINT_STATE(f)
| (FSM) Print the current FSM state information
#define | LIGHT_BAR (_inverted ? 0 : 0xFF)
| Turn display column to all LEDs on.
#define | EMPTY_BAR (_inverted ? 0xFF : 0)
| Turn display column to all LEDs off.
#define | DATA_BAR(d) (_inverted ? ~d : d)
| Turn display column to specified data.
#define | ZE_SET(b, mask) ((b & ~mask) | mask)
| clear the bit then put it back in
#define | ZE_RESET(b, mask) (b & ~mask)
| clear the bit
#define | ZE_TEST(b, mask) ((b & mask) != 0)
| mask off the bit
#define | ZE_FLIP_UD_MASK 0x01
| mask bit 0
#define | ZE_FLIP_LR_MASK 0x02
| mask bit 1
#define | SFX(s) ((_moveIn && _effectIn == (s)) || (!_moveIn && _effectOut == (s)))
| Effect is selected if it is the effect for the current motion.

## Detailed Description

Contains internal library definitions.